=======================================================

SOFTWARE RELEASE NOTE 

=======================================================

PRODUCT:	Professional GP300 / GM300 Series CPS

KIT No.:	PMVN4039L, PMVN4040L (Asia English)

VERSION:	R03.06.07  
DATE OF BUILD:	21-Sep-2006
WEB ACCESS:	Compass website
		http://compass.mot.com/go/210327000

CONTACT:	Xiong Tao
Mail:		a17096@motorola.com
Phone:	        +86-28-8782-6088 Ext. 2306

=======================================================

               Purpose of this release

=======================================================
CPS release supporting Portable and Mobile versions of
the Professional GP300/GM300 Series 5-tone radios.

Supported radio models:
GP320, GP329 (-Plus), GP339 (-Plus), GP340, GP344, 
GP360, GP380, GP388, GP366R 
GM340, GM360, GM380, GM339, GM399, PRO5250, PRO7250

Supported RF bands:
LB1, LB2, LB3, 300, VHF, UHF1, UHF2

=====================
NEW FEATURES / NOTES
=====================
NEW FEATURES:

RGPRG00000121: CCB302 enhancement for Raio ID & Smart PTT

Description:
(1)Support Radio ID feauture:
   In "Per Radio"->"Miscellaneous"->"Global" sheet, a "Radio ID" edit box is added. User can input "Radio ID" digits by this field. 
(2)Refers to Radio ID variables in encode sequence and decode sequence:
   Users can use the formatted string "(U1)", "(U2)", ..., "(U8)" to refers to the separate "Radio ID" digit.
(3)Adding Smart PTT Keyup Mode feature
   a)In "Per Radio"->"Miscellaneous"->"Timers" sheet, a "Smart PTT Periodic Timer" control is added. User can set the timer value by this control.
   b)In "Per Personality"->"Per Personality - N"->"PTT" sheet, add "Smart PTT" item into "PTT Keyup Mode" drop list.And add another two fields "Repeater Access and Radio ID Telegram", "Radio ID Telegram".User uses these two fields to input related telegram index.
(4)Backward compatibility:
   All the new feature is avalible in the case that codeplug version is >= R06.00

RGPRG00000143: CCB290 enhancement for adding IP67 capability into Aoba

Description:
    Add IP67 capability into Aoba (Minnow) to support new model 'Minnow Preferred with Limited Keypad':
    PMUD2236A(H38KDF9AN5), PMUE2779A(H38RDF9AN5) and PMUE2781A(H38SDF9AN5).
    
FIXED THE FOLLOWING ISSUES:

RGPRG00000234: Upgrade issue, CPS set the signalling System with wrong value after Upgrading
Description:
After Upgrading the codeplug archive file,cps set the signalling system with wrong value. please see the attachment.

RGPRG00000248: updated denpendency upon repeater talkaround feature of channel
Description:
Allow user to enable repeater talkaround feature, When talkaround is assinged to programmable button Or when talkaround is enabled on menu.
            
Supports all existing radio versions in the field as well
as the new radio versions.

A ComTool is installed into the same directory as the
CPS, to help customers having problems to access the 
radio via the Com port. The tool gives a detailed 
error message and gives many hints in the file
ComTool.txt how to solve the problem.

NOTE: If using the CPS mail menu, ensure that the last 
changed data is saved to file.

It is possible to keep several CPS version on the 
computer. If only the latest version should be used,
Uninstall any old CPS version before you install the
new one.


=======================================================

         How to install and run this release

=======================================================
Hard disk installation:
---------------------
WEB ACCESS:	Compass website
		      http://compass.mot.com/go/210327000
Download the install package from the Compass website.
Start the installation by running the install package.
========================================================
Disk installation:
------------------
The files for the CPS disks downloaded from the WEB
are PKZIPed. These should be saved on your hard disk in separate
directories and then PKUNZIPed.

Copy the PKZIPED files disk_1, disk_2, disk_3, disk_4 to separate 
directories and unzip it. 

The extracted files should then be copied onto 1.44MB floppies,
except the README and the ZIP file. Label the disks to
disk_1, disk_2, disk_3, disk_4.

Uninstall any previous builds of the same CPS from the PC.

As the CPS is compressed it should be installed from
floppy disk.
With the DISK1 floppy in drive A type:

    'A:\SETUP' for installation 
=========================================================================
