Operation CHARM: Car repair manuals for everyone.

# A/T/Drivetrain - Axle Shaft Component Serviceability

GROUP
TRANS
NUMBER
047
MODEL
All Models
w/ 6-speed A/T
DATE
January 2013
SUBJECT:
AXLE SHAFT SERVICEABILITY BY MODEL
This bulletin provides information regarding axle shaft serviceability for Kia vehicles equipped with a six speed automatic transmission. Refer to the table below for a detailed list of vehicle models. Individual service parts such as axle boots, joints, and hardware for inner joint are now available through your parts department.
1. Remove the axle from the vehicle by referring to the appropriate section of the service information on KGIS.
2. Remove both clamps from the inner tripod joint boot (transaxle side) using a flat-bladed tool, as shown.
3. Carefully slide the boot along the driveshaft and away from the tripod joint. Clean excess grease from the assembly using a shop towel.
4. Carefully remove retaining clip (C) (if equipped) from tripod joint case (B) using snap-ring pliers or an equivalent tool.
5. Separate the tripod joint case from the assembly.
6. Using snap-ring pliers, or an equivalent tool, carefully remove the snap ring (A) from the driveshaft, as shown.
7. Carefully remove the trunnion assy. (B) from the driveshaft (A) using a suitable puller. Use a shop towel to remove any excess grease.
8. Use a small brush to apply a light coating of McLube MoS2-4OO high temperature grease onto splines.
9. Replace all affected parts and reassemble the axle by reversing the order of removal.