Operation CHARM: Car repair manuals for everyone.

# 60000 MI or 96000 KM

Check
Fuel
Check with customer to see if top tier detergent fuel is being used - if not, one bottle of additive is recommended. Do not mix other additives
Inspect
Valve Clearance
Perform at mileage interval or every 48 months, whichever comes first. Inspect engine for excessive valve tappet noise and/or engine vibration and adjust if necessary.
Suspension
Inspect suspension mounting bolts for looseness or damage (tighten to specified torque) at mileage interval or every 12 months, whichever comes first.
Steering
Inspect steering box, linkage, and boots for damage or looseness at mileage interval or every 12 months, whichever comes first. More frequently under driving conditions C, D, E, F, G, H and I
Refrigerant
Inspect at mileage interval or every 12 months, whichever comes first.
Parking Brake System
Inspect the parking brake including the lever (or pedal) and cables at mileage interval or every 12 months, whichever comes first.
Fuel Tank
Inspect fuel tank at mileage interval or every 24 months, whichever comes first.
Fuel Supply Line
Inspect fuel lines, hoses, and connections for damage or leakage at mileage interval or every 24 months, whichever comes first.
Fuel Filter
Perform at mileage interval or every 24 months, whichever comes first.
Fuel Filler Cap
Inspect fuel cap at mileage interval or every 24 months, whichever comes first.
Exhaust System
Inspect exhaust pipe, muffler, and hangers for damage at mileage interval or every 12 months, whichever comes first.
Evaporative Emissions Hose
Inspect fuel vapor lines for damage at mileage interval or every 24 months, whichever comes first.
Evaporative Canister Filter
Inspect fuel tank air filter at mileage interval or every 24 months, whichever comes first.
Emission Control Systems
Inspect vacuum hoses for deterioration at mileage interval or every 6 months, whichever comes first.
Drive Belt
Inspect initially at 60,000 miles or 48 months, whichever comes first. Thereafter, perform every 15,000 miles or 12 months, whichever comes first. Replace if necessary.
Disc Brake System
Inspect disc brake pads, calipers and rotors every 15,000 miles or 12 months, whichever comes first. Inspect more frequently under driving conditions C, D, E, F, G, H and I.
Constant Velocity Joint
Inspect drive shafts and boots for damage. Perform at mileage interval or every 6 months, whichever comes first under conditions C, D, E, F, G, H, I, or J.
Clutch Fluid
Inspect clutch fluid level and condition at mileage interval or every 24 months, whichever comes first - if equipped.
Brake Hose/Line
Inspect for leakage and damage at mileage interval or every 12 months, whichever comes first.
Brake Fluid
Inspect brake fluid level and condition at mileage interval or every 24 months, whichever comes first.
Ball Joint
Inspect dust boots and joints for damage. Perform at mileage interval or every 12 months, whichever comes first. Inspect more frequently if driving under conditions C, D, E, F, G, H or I.
Replace
Oil Filter, Engine
Perform at mileage interval or every 6 months, whichever comes first if driving under conditions A, B, C, D, E, F, G, H, I or K.
Fluid - A/T
Perform at mileage interval or every 48 months, whichever comes first if driving under conditions A, C, E, F, G, H, or I. Replace every 60,000 miles under conditions A, C, E, F, G, H and I, if equipped.
Engine Oil
Perform at mileage interval or every 6 months, whichever comes first if driving under conditions A, B, C, D, E, F, G, H, I or K.
Cabin Air Filter / Purifier
Perform at mileage interval or every 12 months, whichever comes first. Replace more frequently if driving under conditions C or E.
Air Filter Element
Perform at mileage interval or every 24 months, whichever comes first. Replace more frequently as necessary if driving under conditions C or E.
Rotate
Tires
Rotate and inspect tire pressure and tread wear. Perform at mileage interval or every 6 months, whichever comes first.