Operation CHARM: Car repair manuals for everyone.

# 60000 MI or 96000 KM

Check
Fuel
Check with customer to see if top tier detergent fuel is being used - if not, one bottle of additive is recommended. Do not mix other additives
Inspect
Valve Clearance
Inspect for valve noise and/or engine vibration and adjust if necessary. Perform at mileage interval or every 48 months, whichever comes first.
Suspension
Inspect suspension mounting bolts for looseness or damage (tighten to specified torque) at mileage interval or every 12 months, whichever comes first.
Steering
Inspect steering box, linkage, and boots for damage or looseness at mileage interval or every 12 months, whichever comes first.
Refrigerant
Inspect at mileage interval or every 12 months, whichever comes first.
Parking Brake System
Perform at mileage interval or every 12 months, whichever comes first.
Fuel Tank
Inspect fuel tank at mileage interval or every 24 months, whichever comes first.
Fuel Supply Line
Inspect fuel lines, hoses, and connections for damage or leakage at mileage interval or every 24 months, whichever comes first.
Fuel Filter
Perform at mileage interval or every 24 months, whichever comes first.
Fuel Filler Cap
Perform at mileage interval or every 6 months, whichever comes first.
Exhaust System
Inspect exhaust pipe, muffler and hangers for damage at mileage interval or every 12 months, whichever comes first.
Evaporative Emissions Hose
Inspect fuel vapor hoses for damage at mileage interval or every 24 months, whichever comes first.
Evaporative Canister Filter
Inspect the fuel tank air filter at mileage interval or every 24 months, whichever comes first.
Emission Control Systems
Inspect vacuum hoses for deterioration at mileage interval or every 6 months, whichever comes first.
Drive Belt
Inspect drive belt(s) (auto-tensioner, generator, p/str'g, a/con, w/pump) initially at 60,000 miles or 48 months then, every 15,000 miles or 12 months, whichever comes first.
Disc Brake System
Inspect disc brake pads, calipers and rotors every 15,000 miles or 12 months, whichever comes first.
Constant Velocity Joint
Inspect drive shafts and boots for damage at mileage interval or every 12 months, whichever comes first.
Clutch Fluid
Inspect clutch fluid level and condition at mileage interval or every 24 months, whichever comes first - if equipped.
Brake Hose/Line
Inspect for leakage and damage at mileage interval or every 12 months, whichever comes first.
Brake Fluid
Inspect brake fluid level and condition at mileage interval or every 24 months, whichever comes first.
Ball Joint
Inspect dust boots and joints for damage. Replace, if necessary. Perform at mileage interval or every 12 months, whichever comes first.
Replace
Oil Filter, Engine
Perform at mileage interval or every 6 months, whichever comes first.
Engine Oil
Perform at mileage interval or every 6 months, whichever comes first.
Cabin Air Filter / Purifier
Replace climate control air filter (if equipped) at mileage interval or every 12 months, whichever comes first.
Air Filter Element
Replace engine air cleaner element at mileage interval or every 24 months, whichever comes first.
Rotate
Tires
Inspect tire pressure and tread wear. Perform at mileage interval or every 12 months, whichever comes first.