Operation CHARM: Car repair manuals for everyone.

# 127500 MI or 204000 KM

Check
Fuel
Check with customer to see if top tier detergent fuel is being used - if not, one bottle of additive is recommended. Do not mix other additives
Inspect
Emission Control Systems
Inspect vacuum hoses for deterioration at mileage interval or every 6 months, whichever comes first.
Constant Velocity Joint
Inspect drive shafts and boots for damage. Perform at mileage interval or every 6 months, whichever comes first under conditions C, D, E, F, G, H, I, or J.
Air Filter Element
Perform at mileage interval or every 6 months, whichever comes first.
Replace
Oil Filter, Engine
Perform at mileage interval or every 6 months, whichever comes first if driving under conditions A, B, C, D, E, F, G, H, I or K.
Engine Oil
Perform at mileage interval or every 6 months, whichever comes first if driving under conditions A, B, C, D, E, F, G, H, I or K.
Rotate
Tires
Rotate and inspect tire pressure and tread wear. Perform at mileage interval or every 6 months, whichever comes first.