Operation CHARM: Car repair manuals for everyone.

# 142500 MI or 228000 KM

Check
Fuel
Check with customer to see if top tier detergent fuel is being used - if not, one bottle of additive is recommended. Do not mix other additives
Inspect
Emission Control Systems
Inspect vacuum hoses for deterioration at mileage interval or every 6 months, whichever comes first.
Air Filter Element
Perform at mileage interval or every 6 months, whichever comes first.
Replace
Oil Filter, Engine
Perform at mileage interval or every 6 months, whichever comes first.
Engine Oil
Perform at mileage interval or every 6 months, whichever comes first.
Rotate
Tires
Inspect tire pressure and tread wear. Perform at mileage interval or every 12 months, whichever comes first.