Operation CHARM: Car repair manuals for everyone.

# Routine Service

MAINTENANCE FOR OFF-ROAD DRIVING
Frequent maintenance of the following is required whenever the vehicle is driven off-road through mud, water or sand:
- Air cleaner filter
- Brake lining and drums
- Brake lines and hoses
- Brake pads and discs
- Clutch housing
- Differential, transaxle and transfer oil
- Drive shafts and halfshafts
- Steering linkage
- Wheel bearing grease and free running hub grease
CHANGING ENGINE OIL
Use engine oil of proper viscosity only. Always use SG or SH designated engine oil.
EVERY 12 MONTHS
Inspect
Air Conditioning
Refrigerant and compressor operation.
EVERY 10 YEARS
Inspect
Air Bag (SRS System)